Universal Monitor and Control Change Log

May 9, 2019 Version 6.3.3			Bug Fix
1.	Fixed some licensing issues with National Instruments.
2.	Limited to 30 dB gain adjustment abilities to Module firmware version 673.

April 16, 2019 Version 6.3.2			Bug Fix
1.	Rackmount N+1 System Forward and Reflected RF units weren’t displayed properly when the user switched between dBm and Watts.
2.	Added 30 dB gain adjustment support for the compacts.

October 11, 2018 Version 6.2.6		Bug Fix
1. Fixed a bug that was crashing the Universal M&C Installer.

June 14, 2018 Version 6.2.0			Feature Release
1. Added the “Mute Pol 1 Only” and “Mute Pol 2 Only” mute settings to the RCP.
2. Changed the RCP Unmute setting from a 1 to a 255 due to a protocol correction.

April 25, 2018 Version 6.1.1			Bug Fix
1. Fixed some issues with the Compact Outdoor local file locations.

February 21, 2017 Version 4.9.6		Feature Release
1. Added the Switch Mute function to the Compact with Firmware Version 654 and above.

February 10, 2017 Version 4.9.5		Feature Release
1. Removed the Serial number from the RCP Redundant Panels; this was always reporting N/A which was confusing to the users

January 19, 2017 Version 4.9.4		Feature Release
1. Added a Phase Combined 1:2 setting option for the RCP
2. Added a special lock function for the PLOBUC for version 505 and higher
3. Updated the display methods of the internal PLOBUC controls

July 13, 2016 Version 4.9.3			Feature Release
1. Added a menu item for the High Power Outdoor
2. Added a menu item for the Weatherproof units 
3. Fixed some minor issues with the RF Switch faults for the RCP panels
4. Added support for redundant PLOBUC’s

June 9, 2016 Version 4.9.2			Feature Release
1. Updated GUI for PLOBUC
2. Updated Tempco tables for PLOBUC
3. Attenuation updates for the PLOBUC
4. Changed the AutoScaleMode to correct some scaling issues

March 16, 2016 Version 4.9.1			Feature Release
1. Added PowerMAX options for RCP
2. Added HPA Control Panel to RCP. This holds most settings and                                information in a centralized location
3. Changes to the PLOBUC system addressing

March 11, 2016 Version 4.9.0			Feature Release
1. PLOBUC – Addition of the PLOBUC
2. Updated the packet structure for older systems
3. Updated the model number display for the PLOBUC
4. National Instrument controls updated to version 15

August 24, 2015 Version 4.8.14		Feature Release
1.	RCP - Added individual Unit Attenuation Offsets to settings GUI.
2.	ZBUC - Added additional sub-bands S and M to C-Band, and 5 additional TBD place holders.
3.	Compact Outdoor / Mini Compact Outdoor – Added “Forward RF Fault Handling – Major Fault In Online Mode Only” and “Forward RF Fault Handling – Major Fault With Mute” to Forward RF Fault Handling settings.
4.	Rackmount - Added “ALC On”, “High RF Major Fault”, “High RF Minor Fault”, “High RF Major Fault With Mute” to Low Forward RF Fault Handling settings. Settings are now “Ignore”, “Low RF Major Fault”, “Low RF Minor Fault”, “ALC On” (v 4.14), “High RF Major Fault”     (v 6.14), “High RF Minor Fault” (v 6.14), and “High RF Major Fault With Mute” (v 6.14). 
5.	Rackmount - The following labels were renamed on the settings tab:
a.	“Low Forward RF Fault Handling” to “Forward RF Fault Handling”
b.	“Low Forward RF Threshold” to “Forward RF Threshold”
6.	Rackmount – The following items were renamed on the “Forward RF Fault Handling drop down list:
a.	“Major Fault” to “Low RF Major Fault”
b.	“Minor Fault” to “Low RF Minor Fault”
7.	Rackmount – Fault tab Low Forward RF fault LED updated to show the corresponding Forward RF Fault Handling selected in settings.

July 14, 2015 Version 4.8.13			Feature Release
1. Updated RCP Conditions tab and added RF Power and DC Current of each SSPA. Existing temperature graphs are changed to text labels to make space for new additions.
2. Added RF Detector Box super user mode. This is only available in case of emergencies.

May 20, 2015 Version 4.8.12			Feature Release
1. Added forms to add a High Power Outdoor SSPA and an Outdoor PowerMAX Controller Box.
2. Fixed an issue with an internal setting on the Rackmount unit type where settings were not being read correctly.
3. Changed RF Detector Box to be accessible to users. Please do not use unless directed by Paradise employees.

April 30, 2015 Version 4.8.11			Bug Fix Release
1. Fixed an issue with Mini CO where the settings tab was locked out and settings could not be changed.

April 14, 2015 Version 4.8.10			Internal Release
1. Added new internal features specific to rabbit equipped RCP units.
2. Added new internal features for modem.
3. Added new SNMP tab for Rackmount units.

April 6, 2015 Version 4.8.9			Internal Release
1. Implemented a feature to send command packets about three times before giving up and removing the packet to be sent. This will allow SNMP communication to continue to read data if the Write Community string is incorrect and a command is sent.
2. Added internal features specific to rabbit equipped Rackmount units.
3. Fixed bug in RCP Settings (SNMP mode) where fault tolerance was not populating correctly.
4. Fixed bug in RCP Settings (SNMP mode) where the extended protocol was not populating correctly.

January 28, 2015 Version 4.8.8		Internal Release
1. Added features to internal ZBUC unit type.

November 4, 2014 Version 4.8.7		Feature Release
1. Implemented universal SNMP tab to be used for products, though currently not available in all products.
2. Changed wording on Redundant Start Up State per direction by Paradise Technical Support.
3. Added Forward RF Fault for Rabbit equipped vBUCs.
4. Modified Search routine so that it does not take as long to find the unit.
5. Added Internal 1:1 Phase Combined Rackmount Redundant panel.

August 13, 2014 Version 4.8.6			Bug Fix Release
1. Fixed issue with Ethernet communication. Before the fix, if multiple network interfaces were available (on Vista/Windows 7 computers) then some users had to change the interface order or priority.

August 6, 2014 Version 4.8.5			Bug Fix Release
1. Fixed Rack Operation Mode 1:2 Phase Combined setting item. Setting was called out at beginning firmware version 499 and is now fixed for availability for 498.

July 29, 2014 Version 4.8.4			Bug Fix Release
1. Added busy error for Paradise protocol. If busy error is encountered, M&C will resend packet until it no longer receives a busy error.
2. Reworked attenuation control on 1:2 redundant panel.

July 25, 2014 Version 4.8.3			Feature Release
1. Added slave low current fault threshold to Compact Outdoor settings tab.
2. Modified Compact Outdoor Status DC Current tooltip to display total DC current, master DC current, and slave DC current.
3. Renamed Compact Outdoor ‘SSPA DC Current’ to ‘Total DC Current’ to avoid confusion within the logger utility.

July 22, 2014 Version 4.8.2			Bug Fix Release
1. Added Unit Connected/Disconnected status to 1:2 Phase Combined Rack.
2. Bug Fix for N + 1 System Forward and Reflected Power (N/A was not correctly being displayed).

July 21, 2014 Version 4.8.1			Feature/Bug Fix Release
1. Fixed tool tip on vBUC High Temperature Alarm Threshold.
2. Implemented a tool tip on the Compact Outdoor High Temperature Alarm. If the alarm is incorrectly set then the font color will turn red.
3. Fixed search feature within Compact Outdoor and Rackmount unit types.
4. Added 1:2 Phase Combined operation mode to Rackmount (starting firmware version 499). * See 4.8.5 fix for firmware version change.
5. Added options 3, 6, and 12 to Rack N+1 Array Size.
6. Added 1:2 Rack FPC units.

June 27, 2014 Version 4.8.0			Feature/Bug Fix Release
1. Implemented Version 2 of the Universal Logger. The logger now supports manipulation of the Y-Axis and recording data to a file.
2. Fixed internal features of Compact Outdoor calibration.
3. Startup routines were modified to fix a problem that occurred where the startup settings file had become corrupted. The system will now delete the corrupted settings file if it cannot be read.

March 21, 2014 Version 4.7.19			Bug Fix Release
1. Fixed a bug where the Monitor and Control would lose communication with a unit if they were successful in changing a setting before settings could properly be queried from the unit.
2. Fixed a bug on an internal current for the Mini Compact Outdoor. This bug does not affect customers.

March 11, 2014 Version 4.7.18			Bug Fix Release
1. Fixed a bug with one setting on the Compact Outdoor internal view.
2. Fixed a bug with assigning the model and serial number to the Mini Compact Outdoor (internal view only).

February 19, 2014 Version 4.7.17		Bug Fix Release
1. Continued to modify layout of Compact Outdoor internal view. 
2. Fixed a bug with one setting on the Compact Outdoor internal view.
3. Fixed a bug with two settings on the Mini Compact Outdoor internal view.

February 14, 2014 Version 4.7.16		Internal Release
1. Changed location of controls on internal view of Compact Outdoor.
2. Modified Mini Compact Outdoor to have same appearance of Settings tab as the Compact Outdoor.
3. Added new internal settings for Mini Compact Outdoor.
4. Combined multiple queries for Mini Compact Outdoor.

February 7, 2014 Version 4.7.15		Internal Release
1. Fixed power supply names on internal Rackmount documentation.
2. Fixed Compact Outdoor forms to load existing unit information.

January 21, 2014 Version 4.7.14		Internal Release
1. Fixed internal serial number assignment for Mini Compact Outdoor.

January 9, 2014 Version 4.7.13		Internal Release
1. Fixed internal Compact Outdoor utility.

December 18, 2013 Version 4.7.12		Bug Fix Release
1. Fixed warning message for IP Settings change – old warning stated amplifier could be harmed and the new warning states you may lose communication with the unit.
2. Fixed issues with internal RF Detector GUI.

December 5, 2013 Version 4.7.11		Feature Release
1. Added local lock out mode. On units equipped with a Local and Remote Control Mode, this feature will prevent unwanted changes through the Universal Monitor and Control program. If you do not want this feature enabled it can be disabled through the preferences window or you can change the Control Mode to remote using the front panel the unit.
2. Settings were added to the Compact Outdoor to support trap setup. These features can be found on the new tab labeled ‘SNMP Settings’.

November 4, 2013 Version 4.7.10		Internal Release
1. Added new unit type to the internal settings viewer.

October 10, 2013 Version 4.7.9		Bug Fix Release
1. Fixed issue with Mini Compact Outdoor Redundant Panel where the panel was incorrectly configuring the Mini Compact Outdoor.

September 20, 2013 Version 4.7.8		Bug Fix Release
1. Fixed search function for Maintenance Switch Controller.
2. Fixed issue where “Connected” and the associated LED were out of synchronization. LED and connected label should now correspond with one another.
3. Added internal notes for printing.

September 11, 2013 Version 4.7.7		Minor Release
1. Added Maintenance Switch Controller as its own unit type.
2. Incorporated the new Maintenance Switch Controller in to the N+1 System. Users can either add a standard Controller or Maintenance Switch Controller for the Maintenance Switch Controller of the N+1 System.
3. Modified the internal GUI for the CO making items easier to find.

September 5, 2013 Version 4.7.6		Minor Release
1. Locked users out of BUC fault status on CO and Mini CO settings.
2. Fixed internal storage facility database functions.

June 28, 2013 Version 4.7.5			Feature Release
1. Added ‘Very Quick Polling’. This option should only be used when communicating with several units.
2. Added Rackmount settings as outlined in latest protocol documents.
3. Added RCP settings as outlined in latest protocol documents.
4. Remodeled the N+1 tab on the Rackmount. Attenuation was added to the panel.
5. Added internal features to Compact Outdoor. 

June 12, 2013 Version 4.7.4			Bug Fix Release
1. Fixed Rackmount sending multiple TCP/IP changes.
2. Fixed Rackmount Board Versioning error.

June 7, 2013 Version 4.7.3			Feature Release
1. Added Very Quick Polling mode.
2. Added Reflected RF Fault for Compact Outdoor units.

May 31, 2013 Version 4.7.2			Feature Release
1. Added more support for advanced N+1 Systems.
2. Fixed an issue with the Compact Outdoor mute button.
3. Added System X and Single Switch options for the Controller.
4. Added Switch Lock, Auto Gain options, and additional conditions for the Rackmount.

April 19, 2013 Version 4.7.1			Feature Release
1. Added support for firmware version 478 in Rackmount M&C.
2. Fixed Rackmount standby indicator in Faults tab.

March 20, 2013 Version 4.7.0			Feature Release
1. Added tool tip when hovering over buttons to change to other units, tool tip will display unit type, model number, and serial number (if communications are present).
2. Modified the Device Tree to be on an expandable panel. This allows you to hide the Device Tree if you do not wish to have it visible.
3. Added Gain Calibration mode to the Settings page on the Compact Outdoor SSPA.
4. Added additional faults and settings to the Rackmount SSPA.
5. Updated the icons from the old Paradise logo to the newer style Paradise logo.
6. Added more configurable options in the Preferences window. Users can now choose their own Source Address and the program now supports proper saving and restoring of the UDP Ports configuration.
7. Window size and Device Tree panel size are now saved appropriately (bug fix). Prior to this version, the window size would not factor in the Device Tree panel size. In addition to this, the program will save the state of the Device Tree panel (expanded or collapsed).

January 17, 2013 Version 4.6.9		Production Release
1. Added tool tip to Protocol Select on Compact Outdoor and Mini Compact Outdoor.

November 29, 2012 Version 4.6.8		Production Release
1. Added new model numbers to Rackmount.
2. Fixed production settings viewer.
3. Added new settings for Compact Outdoor (production only).
4. Fixed bugs on production calibration settings.
5. Added new settings for RCP.

November 12, 2012 Version 4.6.7		Production Release
1. Fixed SNMP Location field.

September 25, 2012 Version 4.6.6		Production Release
1. Internal changes made to vBUC to allow setting of RF Detector table if no database connection exists.

August 21, 2012 Version 4.6.5			Production Release
1. Removed block on reference selection on vBUC (previously determined correct usage based on model number).

August 21, 2012 Version 4.6.4			Production Release
1. Added database connectivity for Storage Facility.

August 21, 2012 Version 4.6.3			Production Release
1. Added Storage Facility for internal use.

August 8, 2012 Version 4.6.2			Feature Release
1. Added Mini CO Redundant Panel.

July 27, 2012 Version 4.6.1			Production Release
1. Added Configuration Single Switch and System Type SystemX to RCP.
2. Added System Operation Mode 1:1 Phase Combined and N+1 Array Size 2 for the Rackmount.

June 18, 2012 Version 4.6.0			Feature Release
1. Added SNMP support to the Compact Outdoor SSPA, Mini Compact Outdoor SSPA, Rackmount SSPA, Controller, and vBUC unit types.
2. Added a fan speed adjustment for the Compact Outdoor SSPA unit type (please review your manual before changing any settings through the Universal Monitor and Control program).
3. Removed the ‘System Configuration” selection from the ‘Add Controller’ window. The system is automatically queried and will update the screen graphics upon receiving this data from the system. 

January 31, 2012 Version 4.5.3		Bug Fix Release
1. Fixed a bug on the Controller and Rackmount units where an error message would prevent you from opening the unit in the M&C.
2. Changed the Windows Imaging Component to be a separate install. This will only affect Windows XP users running Service Pack 2. It is recommended that you upgrade to Service Pack 3.
3. Fixed a bug with the Query Timer. Previously a change in the Query Timer would not result in the appropriate change.

December 14, 2011 Version 4.5.2		Production Release
1. Added Windows Imaging Component prerequisite to the installer.

September 23, 2011 Version 4.5.1		Production Release
1. Added RF Detector Box for internal use (database support).

June 23, 2011 Version 4.5.0			Production Release
1. Updated N+1 PowerMAX panel to N+1 System panel.
2. Changed to .Net 4.0.
3. Added 64 bit compatibility.

May 5, 2011 Version 4.4.15			Bug Fix Release
1. Fixed RCP to allow Firmware Version 43I.

April 20, 2011 Version 4.4.14			Production Release
1. Added Rackmount Fan Speed for Firmware Version 443 or higher (replaces LCD Intensity).
2. Added Rackmount Auxiliary Fault Handling Minor Fault with Mute for Firmware Version 443 or higher.
3. Replaced Rackmount numeric editing controls for custom controls which increase reliability.
4. Added additional Ka ZBUC support for production level testing.
5. Adjusted vBUC tables for production support.

February 28, 2011 Version 4.4.13		Bug Fix Release
1. Fixed Rackmount versioning. Conditions query length changed from version 420 to version 423.

October 11, 2010 Version 4.4.12		Feature Release
1. Added Mini Compact Outdoor SSPA support.
2. Fixed bug on internal Protocol debugger using Ethernet communications.
3. Updated Help file with PowerMAX and Mini Compact Outdoor SSPA section.
4. Changed name from Paradise Datacom LLC to Teledyne Paradise Datacom.

August 16, 2010 Version 4.4.11		Bug Fix Release
1. Fixed PowerMAX power reporting 10x less.

August 10, 2010 Version 4.4.10		Production Release
1. Fixed PowerMAX system settings printer.

August 6, 2010 Version 4.4.9			Production Release
1.	Fixed PowerMAX model number scheme.

June 9, 2010 Version 4.4.8			Bug Fix Release
1. Fixed PowerMAX system connected/disconnected status.

June 3, 2010 Version 4.4.7			Production Release
1. Implemented production features for Master/Slave CO.
2. Added Ka ZBUC for production level testing.

April 28, 2010 Version 4.4.6			Bug Fix Release
1.	Modified EEprom fault to signify Fiber Fault as well.
2.	Fixed vBUC mute setting from 1 to 255 (see protocol).

March 18, 2010 Version 4.4.5			Feature Release
1.	Added PowerMAX support using Rack and PowerMAX panels.

November 12, 2009 Version 4.4.4		Bug Fix
1. Added Online/Standby indicator on Compact Outdoor M&C.
2. Fixed CO Spare Fault Wizard (Forward RF Power, Gate Voltage).

October 2, 2009 Version 4.4.3			Feature Release
1. Added SNMP protocol select to Compact Outdoor M&C.
2. Added Forward RF Fault to Compact Outdoor M&C (Firmware Version 500+).

September 25, 2009 Version 4.4.2		Feature Release
1. Added IP Net protocol select to Compact Outdoor M&C.

July 27, 2009 Version 4.4.1			Feature Release
1. Removed pass-through communication ability from Compact Outdoor M&C.

June 2, 2009 Version 4.4.0			Feature Release
1. Fixed text on various panels.
2. Added option fault on Rack Mount GUI.
3. Changed prereq of .NET Framework 3.5 to 2.0 and included in installer.
4. Added Evo Modem testing for production use.

July 14, 2008 Version 4.3.3			Feature Release
1. Fixed vBUC spare fault settings.

July 2, 2008 Version 4.3.2			Bug Fix Release
1. Fixed vBUC low current setting.
2. Fixed vBUC redundancy panel.

June 6, 2008 Version 4.3.1			Production Release
1. Fixed Universal Logger.
2. Updated Universal M&C help.

June 2, 2008 Version 4.3.0			Production Release
1. Added read and write community strings.
2. Added feature to pull system settings upon reconnect.
3. Added vBUC to available products.
4. Fixed mute on reconnect issue with Rack SSPA.

December 18, 2007 Version 4.1.0		Production Release
1.  Added pass through support for Compact Outdoor.
2.  Fixed VSAT 3100 power class to show a power class of zero. 	

September 20, 2007 Version 4.0.8		Production Release
1.  Fixed carrier enable/mute issue with Compact Outdoor.
2.  Added LNA LNB Switching Voltage to RCP.
3.  Fixed MAC address assignment.
4.  Added additional tools for factory use.
5.  Added feature to Rack SSPA to restore settings, MAC address, etc from file.
6.  Added external mute condition on Compact Outdoor Status tab.

July 17, 2007 Version 3.2.2			Production Release

June 21, 2007 Version 3.2.1			Bug Fix
1.  Fixed compatibility issue with other Paradise Datacom Applications.

May 25, 2007 Version 3.2			Feature Release
1.  Fixed maximized window resize bug.

March 16, 2007 Version 3.1			Feature Release
1.  Updated unit calibration feature
2.  Implemented new layer in code architecture for flexible version upgrade.

March 6, 2007 Version 3.0.3			Feature Release
1.  Added recognition for external mute in Compact Outdoor
2.  Fixed decimal point error in Low Current Fault Threshold value

February 2, 2007 Version 3.0.2		Feature Release
1.  Added TCP/IP capabilities to RCP units.
2.  Made Serial Number Utility accessible to RCP and Rackmount units
3.  Added Uniform LED On/Off colors
4.  Fixed tree view context menu bug
5.  Added descriptive tab page naming
6.  Adjusted logger GUI to prevent bugs
7.  Adjusted automatic tab page numbering system
8.  Fixed controls issue on Compact status page

August 29, 2006 Version 2.5.3			Feature Release
1.  Added necessary features to configure IP Enabled
Digital Core Board 4 in the factory.

July 25, 2006 Version 2.5.1			Bug Fix Release
1.  Added more verbose messaging to Serial Number Utility.

July 25, 2006 Version 2.5.0			Feature Release
1.  Serial Number utility updated for factory use.

June 30, 2006 Version 2.4.1			Feature Release
1.  Added Reflected Power Calibration to Rack SSPA.
Factory Use Only.
2.  Added Serial Number and MAC Address dispenser to
Compact Outdoor SSPA.  Factory Use Only.
3.  Added Logger.

February 21, 2006 Version 2.3.2		Feature Release
1.  Modified Internal Redundant Control Panels.  They
now reflect information from SSPAs that the RCP does.
2.  Added functionality for saving and restoring
SSPA calibration data. (Consult Factory)
3.  Added functionality for Auto-Loading last device
configuration at start-up.

December 14, 2005 Version 2.3.0		Feature Release
1.  Added “Print System Settings” to Compact Outdoor SSPA
Calibration Tab (Only available at the factory)
2.  Implemented Compact Outdoor SSPA Firmware Ver.350
3.  Upgraded Internal 1:1 Status Panel
4.  Upgraded RCP2 Status Panels

August 16, 2005	Version 2.2.0		Bug Fix Release
1.  Fixed logic that would block new values committed in
Comboboxes from being sent to the remote device.
2.  Fixed waveguide switch logic in FPRC-1100 switch 2.
3.  Fixed RCP search bug.
4.  Fixed multiple baud rates on single com port bug.
5.  Fixed VSAT BUC baud rate exception due to serial
engine switch.

July 7, 2005	Version 2.1.1		Feature Release
1.  Added protocol additions to RCP2.  New additions include
dBm or Watts power units selection, SSPA and Ambient
Temperature display and Reflected Power Monitor.

July 1, 2005	Version 2.1.0		Bug Fix Release
1.  Fixed bug that would disallow using 0 for the network
Address of the device.

May 9, 2005		Version 2.0.0		Feature Release
1.  Removed National Instruments VISA Runtime.  
Replaced with OpenNETCF serial engine.  Source code 
For the serial engine is available upon request.
2.  Removed tab control on main GUI and replaced with
preferences form in Action->Preferences menu.
3.  Additions for Factory Alignment and Calibration.

March 10, 2005	Version 1.4.0		Bug Fix Release
1.  Made changes to Serial and UDP engines for more
robust communications.
2.  Made cosmetic changes to SplashScreen.
3.  Fixed bug that forced baud rate to 9600 for
Serial devices.
4.  Added Combine button on FPRC-1100 version of
RCP2 M&C.
5.  Fixed Waveguide Switch 2 logic on FPRC-1100
Version of RCP2 M&C

December 8, 2004	Version 1.3.1	Bug Fix Release
1.	Fixed bug that wouldn’t allow Rackmount SSPA
to update IP Settings when connected Serially.
2.  Allow “Enter” button to change values in numeric
Controls on Compact Outdoor, Rackmount and VSAT BUC
status panels.

November 29, 2004	Version 1.3.0	Production Release
1.  Multiple device configurations are now allowed.
2.  Device configuration files are now saved in 
SOAP XML format.
3.  Legacy configuration file is converted to a file
Called saved.xml.
4.  Fixed bug in 3100 Series BUC that would not
indicate that the device was “Connected”.

November 17, 2004	Version 1.2.2	Bug Fix Release
Bug from 1.2.1 in Disconnect indicator fixed.  Unit would
never recover from Disconnect condition.

October 27, 2004	Version 1.2.1	Bug Fix Release
1. Fixed Bug in Serial Engine that would not allow two 
units to share the same serial communication port.
2. Fixed Bug in Core M&C that miscalculated 2 byte 
return values from remote units.
3. Changed the way that queries are dispatched to 
Remote Units.  Queries are sent one at a time on a 
periodic basis instead of building in a queue and 
sent at the same time.
4. “Port Busy” exception is handled in Load 
Configuration.

July 9, 2004	Version 1.2.0	Production release
Set support email to my personal email address

June 21, 2004	Version 1.1.1	Beta release
Changed NI-VISA runtime from version 3.0.1 to 3.1.0
Refactored System Data Array hierarchy for efficiency

June 14, 2004	Version 1.1.0	Beta release
Added support for RCP2 product line and VSAT BUC 
product line
Fixed bug in Compact Outdoor SSPA GUI that would 
update controls while users were making changes
Fixed Rackmount SSPA software version parsing

April 13, 2004	Version 1.0.2
Fixed location of Help file
Fixed exception where Port was disposed twice
Allow more time for unitSettings GUI's to 
make choice from ComboBox

April 7, 2004  	Version 1.0.1
Fixed Bug in Rack Mount Settings class

April 1, 2004  	Version 1.0		Initial Release